Driver package for Kube 200 dpi printer:

Supported Operative Systems:

Windows XP.
Windows Vista.
Windows 7.
Windows 8.
Windows 8.1.
Windows 10.

Installation procedure:

a) Serial interface
For a serial interface printer you may execute the standard
printer installation procedure or follow the automatic wizard procedure.
For standard printer installation the needed files are stored into: "..\CeTmpDrv" directory.

b) USB interface
Please follow the automatic wizard procedure.


This driver support printer:
"Custom KUBE 82.5mm (200dpi)"

The "Custom KUBE 82.5mm (200dpi)" prints on a paper width size of 82.5mm but the printable
region width is 80mm.

This printer supports the following page formats:

"KUBE Roll 82.5mm"
"KUBE Roll Short 82.5mm"
"KUBE 82.5x82.5mm"
"KUBE 82.5x125mm"
"KUBE 82.5x165mm"
"KUBE 82.5x205mm"
"KUBE 82.5x245mm"
"KUBE 82.5x285mm"
"KUBE 82.5x405mm"

[ the defalut installation page is "KUBE Roll Short 82.5mm" ]

If the system driver properties section shows these format pages and other not here
specified, you must select only the above mentioned pages format.

Note about BlackMark Feature:
 we suggest to use "KUBE Roll" page format when You are using Notch Alignment.

